File Conversion (Resample) | << Prev / Next >>

To resample standard Windows files (*.wav)
Click the [CONVERT] button and select [Resample...] from [Single file]
or [Multiple files]. After selecting the input WAVE file, the Resample setting
dialog box appears. Select the output wave format and start resampling.
This tool converts only PCM-Wave format files. The conversion process takes
a long time, since Sin conversion method is used for resampling. However,
when Quality level is set high, resultant file's quality will be fairly good.
[Cancel] button stop will stop the conversion process.

Resampling Options:

[Wave Info] | ... Shows input file information.
[Sample rate] | ... Sample rate setting for the output file. 2000~96000Hz is available.
[Resolution] | ... Choose between 8bit and 16bit. Select 16bit for encoding.
[Channel] | ... Choose mono or stereo.
[Resample Quality] | ... Set a value from 1 to 100. While a higher value makes better. ... quality sound, it takes longer time.

Batch Resampling
Batch Resampling option performs multiple wave file resampling.
It processes files in the order listed in Resample List. This is useful
when you resample a large number of wave files.
dialog box appears. Select the output wave format and start resampling.
Files are output to the predefined path. You can set different paths for
each file. To set the default path, click on the [Target] column title of
the batch resample window. To initialize the normal output path, click on
the [Source] column title. Clicking on [Quality] column title makes the
quality settings of all files in the list the same as the top file in the list.
Similarly, [Format] column title makes the output format settings of files
in the list the same as the top file.
Output format can be changed by double clicking the file name in the list.

[Add] | ... Adds a file to the resample list.
[Save] | ... No use.
[Clear] | ... Clears the resample list.
[Exit] | ... Exits from the batch resampling process. If you click this button during ... the resampling process, it halts the whole resampling process. ... Before it halts resampling, confirming message appears.
[Start] | ... Starts the batch resampling process.

<< Prev / Next >>